**Dominion PX PX-3420 Tech Specs**



|  |  |
| --- | --- |
| PDF Icon | [Click here for a PDF of the Data Sheet](http://www.raritan.com/products/power-management/px-3000/px-3000-data-sheet.pdf) |
| PDF Icon | [Click here for a PDF of the Mechanical Drawing](http://www.raritan.com/support/dominion-px/Mechanical-Drawing/Case_assy_PX-3420.pdf) |
| PDF Icon | [Click here for a PDF of the Inline Meter Solution Brief](http://www.raritan.com/products/power-management/dominion-px/inline-meters-solution-brief.pdf) |

Input

* Nominal voltage: 100 - 240V AC, single phase
* Maximum current per line: 32A
* Rated current: 32A per line
* Load capacity: 7.7 kVA
* Frequency: 50-60 Hz
* Input type: 4 x AC terminal

Output

* Nominal voltage: 100 - 240V AC
* Current draw: 16A to 32A per line
* Output type: 4 x AC terminal

Metering

* Input: Current, voltage and power for each line
* Output:
  + Current, voltage and power for each outlet and total PDU
  + Current and trip state (on/off) for each circuit breaker

Rack Environment Management

* Optional temperature and humidity sensors (RJ-12 connector)

Interface and Protocol Support

* 10-100 Mbps Ethernet (RJ-45 connector)
* RS-232 serial (RJ-45 connector)
* SNMPv2, v3 TRAPs, GETs, SETs
* Web browser and command line interface access

Mechanical

* Rack space: 1U
* Mounting: Rack mount brackets included
* Dimensions (WxDxH): 17.3" x 11.3" x 1.7"; 440 x 287 x 44mm
* Weight: 10.6 lbs; 4.8 kg
* Color: Black powder coat
* Shipping dimensions (WxDxH):
* Shipping weight:  lbs;  kg

Environmental Requirements

* Operating temperature: 5-60 degrees Celsius
* Humidity: 5-90% RH non-condensing
* Altitude: 10,000 feet

Approvals

* FCC Part 15, A; UL and c-UL 60950
* RoHS compliant

Warranty

* Two years, 100% parts and workmanship