**Dominion PX PX-5469 Tech Specs**



|  |  |
| --- | --- |
| PDF Icon | [Click here for a PDF of the Data Sheet](http://www.raritan.com/products/power-management/px-5000/px-5000-data-sheet.pdf) |
| PDF Icon | Click here for a PDF of the Mechanical Drawing |

Input

* Nominal voltage: 230V AC
* Maximum line current per phase: 32A
* Rated current: 32A per phase
* Load capacity: 7.4 kVA
* Frequency: 50-60 Hz
* Plug type: IEC 60309 32A

Output

* Nominal voltage: 208V AC
* Maximum current draw: 16A per circuit
* Switched receptacles: 16 x IEC C-13, 4 x IEC C-19
* Overload protection: 2 x 16A single-pole UL489 circuit breakers

Metering

* Input: Current, voltage and power for each line
* Output:
	+ Current, voltage and power for each outlet and total PDU
	+ Current and trip state (on/off) for each circuit breaker

Rack Environment Management

* Optional temperature and humidity sensors (RJ-12 connector)

Interface and Protocol Support

* 10-100 Mbps Ethernet (RJ-45 connector)
* RS-232 serial (RJ-45 connector)
* SNMPv2, v3 TRAPs, GETs, SETs
* Web browser and command line interface access

Mechanical

* Rack space: Zero U
* Mounting: Rack mount brackets included
* Dimensions (WxDxH): 2.1" x 2.6" x 60.6"; 52 x 65 x 1539mm
* Weight: 14.1 lbs; 6.4 kg
* Display panel: LED for PDU and outlet current and voltage
* Line cord: 10 ft / 3 m
* Color: Black powder coat
* Shipping dimensions (WxDxH): 10.2" x 5.1" x 73.3", 260 x 129 x 1860mm
* Shipping weight: 18.5 lbs; 8.4 kg

Environmental Requirements

* Operating temperature: 5-40 degrees Celsius
* Humidity: 5-90% RH non-condensing
* Altitude: 10,000 feet

Approvals

* FCC Part 15, A; UL and c-UL 60950
* RoHS compliant

Warranty

* Two years, 100% parts and workmanship