**Dominion PX PX2-1190R Tech Specs**

|  |  |
| --- | --- |
| PDF Icon | [Click here for a PDF of the Data Sheet](http://www.raritan.com/products/power-management/px-1000/px-1000-data-sheet.pdf) |

 Input

* Nominal voltage: 230V AC
* Maximum line current: 16A
* Rated current: 16A
* Load capacity: 3.7 kVA
* Frequency: 50-60 Hz
* Plug type: IEC60309 16A

Output

* Nominal voltage: 230V AC
* Maximum current draw: 20A
* Unswitched receptacles: 8 x IEC C-13

Metering

* Inlet: Kilowatt hours (kWh), current (Amps), voltage, power (kVA, kW), power factor

Rack Environment Management

* Optional temperature and humidity sensors (RJ-12 connector)

Interface and Protocol Support

* 10-100 Mbps Ethernet (RJ-45 connector)
* RS-232 serial (DB9 connector)
* Feature/KVM (RJ-45 connector)
* USB-A (host), USB-B (device)
* SNMPv2, v3 TRAPs, GETs, SETs
* Web browser and command line interface access

Mechanical

* Rack space: 1U
* Mounting: Rack mount brackets included
* Dimensions (WxDxH): 17.3" x 5.2" x 1.7"; 440 x 133 x 44mm
* Weight: 7.8 lbs; 3.6 kg
* Display panel: Autoflip LED for PDU current (A), voltage, power (kW)
* Sensor indicator
* Line cord: 10 ft / 3 m
* Color: Black powder coat
* Shipping dimensions (WxDxH): 22.8" x 17.2" x 14.0"; 580 x 437 x 355mm
* Shipping weight: 10.7 lbs; 4.9 kg

Environmental Requirements

* Operating temperature: 5-60 degrees Celsius
* Humidity: 5-90% RH non-condensing
* Altitude: 10,000 feet

Approvals

* FCC Part 15, A; UL and c-UL 60950
* RoHS compliant

Warranty

* Two years, 100% parts and workmanship